SPECS: 300 Narragansett Ave., Barrington, RI 02806

House in AE zone; one corner of lot in VE Zone

--AE does NOT require breakaway walls, just a flow-through Styrofoam or other door.

Elevation: first living floor should be 10Ft above mean high tide (ground level)

--on concrete walls with a pier system and steel beams in garage level

Exterior Walls: white cedar shingle

Windows: Anderson

Exterior moldings, trim: natural or French blue stain

Shutters: French blue

Floors: hardwood (light oak) except ceramic tile in bathroom

Cabinets: maple

Countertops: Formica, unless otherwise specified

Heat: gas fired hot air—in attic

Air conditioning: gas-fired—in attic

Hot water: on first floor (bathroom), gas-fired
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