SEPTEMBER 4, 2000

1. ALL FLOORS HARDWOOD EXCEPT AREAS MARKED “FOYER”, WHICH ARE TO BE TILE. EXCEPTION IS GARAGE LEVEL (GARAGE SLIP AND “UNFINISHED” AREA).

2. ALL WOODWORK IS TO BE STAINGRADE AND FINISHED WITH STAIN AND POLYURETHANE.

3. ALL WINDOWS MUST BE APPROVED BY J. BILLSON BEFORE INSTALLATION.

4. IN PREPARING BLUEPRINTS, NO CHANGES TO BE MADE FROM FLOOR PLANS AND ELEVATIONS PROVIDED SEPT. 4, 2000, WITHOUT APPROVAL OF J. BILLSON.

